**Technical characteristics**

|  |  |
| --- | --- |
| Volume of inspired gas, ml, not less than | 900 |
| Capacity of ventilation bag, ml | 1650±200 |
| Capacity of reservoir bag ml | 2600 |
| Minute ventilation, l/min | 31 |
| Pressure limitation in breathing circuit, hPa | 55±15 |
| Resistance to inspiration, hP | 5 |
| Resistance to expiration, hPa | 2 |
| Gas leak at pressure 30hPa, l/min, not more than | 0,5 |
| Overall dimensions, mm (in a cover bag) | 350х140х200 |
| Weight, kg | 0,9 |